**Acrylic Electrical Enclosure**:

All parts to be cut out on laser bed out of 1/8” clear Acrylic. No need to account for screw holes and wire passthroughs. These can be added by the team later during assembly.

|  |  |  |
| --- | --- | --- |
| **Part** | **Quantity** | **Dimensions (Inches)** |
| Back | 1 | 5.25 X 9.75 |
| Front | 1 | 5.5 X 11.0 |
| Lid | 1 | 10 X 15.25 |
| Side | 2 | 5.375 X 16.25 |
| Bottom | 1 | 9.75 X 16.25 |
| Triangular Bracket | 8 | 1.0 X 1.0 (x and y of right triangle) |

We would like to have a 4” X 4” cougar logo cut into the Lid centered at (5.0” , 7.625”). This will serve as a decorative vent feature.